**VENTURIMETER**

**INTRODUCTION:**

The Ventura meter used in this experiment consists of successive converging, uniform and diverging sections equipped with pressure taps at selected locations.

A Ventura meter is a device for determining the flow-rate of a fluid down a pipe. One measures the pressure difference between the venture inlet and neck, and from this the flow-rate can be determined.

**OBJECTIVE:**

To study the variation of Cod and discharge with respect the head by plotting the following graphs


Vs

Vs h

Taking and h on x-axis and on y-axis

**THEORY:**

Venturimeter is a device used for measuring the rate of flow of a fluid through a pipe. Water is allowed to flow through the meter at different rates ranging from zero to the maximum and the corresponding pressure differences shown in the manometer are noted. The actual discharge A is determined using the measuring tank and the stop watch.



Actual discharge (A) = a x h/t m3/s

Where


a – Area of measuring tank in cm2

h – Height differences in pyrometer in cm

t – Time to collect water for a height difference of h cm, measured in

Seconds

Theoretical discharge is given by



Where

A1 – The area at inlet side in cm2

A2 – The area at throat in cm2

Hw – Head difference in the manometer, converted to cm of water

g – Acceleration due to gravity (9.81 m/sec²)

Coefficient of discharge is given by

image6.png

**OBSERVATIONS AND CALCULATIONS:**

Plan area of the tank A =

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Sl. no** | **Time for 10cm rise of water level (s)** | | | **Actual discharge Acm3/s** | **Differential head in cm. of mercury** | | | **Differential head in cm. of water.** | **Theoretical discharge Qth,cm3/s.** | **Coefficient of discharge Cod** |  |
| **h1** | **h2** | **h1- h2**  **Hug** |  |
| **t1** | **t2** | **tm** |  |
| **1**  **2**  **3**  **4**  **5** |  | | |  |  |  |  |  |  |  |  |

**MANUAL:**

Start the experiment by pressing the start button with keeping default values of inlet die of venturimeter and throat die and rise of water level H and discharge ,then pass the experiment after few cycles and note the observations.

**Observations1:**

1) Allow the water to flow from the inlet or gate valve through the pipe to the convergent cone, then the level of the pyrometer rises up to some height.

2) Then the measure the pressure head in the pyrometer.

**Observation2:**

1) Then allow the water to flow from the convergent to throat and from the throat to the divergent cone.

2) Hen level in the pyrometer rises up to some height. Rising depends upon the rate of flow of water.

**Observation3:**

1) Then allow the water to flow in to the collecting through the outlet and after filling some amount of water in the collecting tank ,the water level in the collecting is increased and the measure the time taken to collect the water for every 10cms rise.

2) Repeat the experiment by changing the discharge, inlet die and throat and rise of water level.

###### RESULT: Coefficient of discharge of venturimetre Cod =

###### MAINTENANCE:

1. After completing the experiment close the inlet valve and open all the gate valves and needle valves to vent any air trapped inside and then close them.

2. Drain the water from measuring tank after completing the experiment.

**QUIZ:**

1. Venturimeter is used to measure average velocity
2. true
3. false
4. Angle of contraction is more than angle of diversion
5. true
6. false
7. The inlet length of the Venturimeter’s greater than outlet pipe
8. true
9. false
10. Actual discharge is obtained by (A)= a x h/t
11. true
12. False
13. Coefficient of discharge is calculated by =

a) True

b) False

**REFERENCE:**

1. FLUID MECHANICS - RK BANSAL
2. EXPERIMENTS ON FLUID MECHANICS - SARABJIT SINGH
3. WIKIPEDIA

The constructor- http://theconstructor.org/